Nameplate to be mounted when ready on the Std. GBE Plaque is 13”W x 15” High, with OGEE edge, as shown below.

GBE face casting is 7-5/8” diameter, set above center on the wooden plate.

Details of engraved plate for basis of award, name and date are shown below.

 OGEE EDGE

For Outstanding Individual Service to the Profession as well as
Leadership and Inspiration in the Development of Civil Engineers

Presented to

**Gary Chock, S.E., F.SEI, F.ASCE, D.CE**

by the

## **Cleveland Section**

**American Society of Civil Engineers**

# October 9, 2014

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

*[The above text is shown at desired font and actual size.]*

*The next page shows how the plaque should look.*

Example how plate should look:

For Outstanding Individual Service to the Profession as well as
Leadership and Inspiration in the Development of Civil Engineers

Presented to

**Henry Petroski**

 by the

## **Cleveland Section**

**American Society of Civil Engineers**

# October 18, 2012

GOLD

BLACK GLOSS BACKGROUND W/ GOLD LETTERS